In order to do a firmware update follow the following steps:

1. Connect to the correct comport and select baudrate.
2. Do a REQ_UD2 (please note that the correct Dongle ID is displayed and the invocation counter is updated).
3. Open the firmware file you want to program (file/open).
4. Program the firmware (options/firmware update).

